From e9fd60840eb125dcd55aab859dd838a47c02931f Mon Sep 17 00:00:00 2001
From: Jeremie Corbier <jeremie+debian@famille-corbier.net>
Date: Tue, 6 Apr 2010 15:51:03 +0200
Subject: [PATCH] Fix manpages

This patch fixes wide-dhcpv6 manpages (paths, typos, ...).

Signed-off-by: Jeremie Corbier <jeremie@famille-corbier.net>
---
 dhcp6c.8      |    8 ++++----
 dhcp6c.conf.5 |    4 ++--
 dhcp6ctl.8    |   13 ++++++-------
 dhcp6relay.8  |    1 -
 dhcp6s.8      |   10 +++++-----
 dhcp6s.conf.5 |    2 +-
 6 files changed, 18 insertions(+), 20 deletions(-)

diff --git a/dhcp6c.8 b/dhcp6c.8
index 6824ae0..1d69c9d 100644
--- a/dhcp6c.8
+++ b/dhcp6c.8
@@ -114,13 +114,13 @@ In either case,
 will send DHCPv6 Release messages to release resources assigned from servers.
 .\"
 .Sh FILES
-.Bl -tag -width /usr/local/etc/dhcp6c.conf -compact
+.Bl -tag -width /etc/wide-dhcpv6/dhcp6c.conf -compact
 .It Pa /var/run/dhcp6c.pid
 is the default file that contains pid of the currently running
 .Nm dhcp6c .
-.It Pa /usr/local/etc/dhcp6c.conf
+.It Pa /etc/wide-dhcpv6/dhcp6c.conf
 is the default configuration file.
-.It Pa /var/db/dhcp6c_duid
+.It Pa /var/lib/dhcpv6/dhcp6c_duid
 is the file to store the client's DUID.
 .El
 .Sh Configuration Script
@@ -203,6 +203,6 @@ command first appeared in WIDE/KAME IPv6 protocol stack kit.
 is incomplete and violates DHCPv6 protocol spec, in several aspects.
 In particular, temporary address assignment is intentionally omitted.
 .Pp
-Information Refresh Time Option is not recognied in Info-req mode, since
+Information Refresh Time Option is not recognized in Info-req mode, since
 .Nm
 terminates after it receives a REPLY message.
diff --git a/dhcp6c.conf.5 b/dhcp6c.conf.5
index 611ab4f..5fc03d3 100644
--- a/dhcp6c.conf.5
+++ b/dhcp6c.conf.5
@@ -36,7 +36,7 @@
 .Nd DHCPv6 client configuration file
 .\"
 .Sh SYNOPSIS
-.Pa /usr/local/etc/dhcp6c.conf
+.Pa /etc/wide-dhcpv6/dhcp6c.conf
 .\"
 .Sh DESCRIPTION
 The
@@ -630,7 +630,7 @@ execute the
 .Xr openssl 1
 command (when available) as follows,
 .Bd -literal -offset
-% openssl rand -base64 16
+% openssl rand \-base64 16
 .Ed
 .Pp
 and copy the output to the
diff --git a/dhcp6ctl.8 b/dhcp6ctl.8
index 86ea0e1..e11889b 100644
--- a/dhcp6ctl.8
+++ b/dhcp6ctl.8
@@ -85,12 +85,11 @@ Use
 .Ar keyfile
 to provide the shared secret to communicate with the process.
 The default file name used when unspecified is
-.Pa /usr/local/etc/dhcp6cctlkey
+.Pa /etc/wide-dhcpv6/dhcp6cctlkey
 with a client,
 and
-.Pa /usr/local/etc/dhcp6sctlkey
+.Pa /etc/wide-dhcpv6/dhcp6sctlkey
 with a server.
-
 .It Fl p Ar port
 Specify
 .Ar port
@@ -99,7 +98,7 @@ The default port number used when unspecified is 5546 for a client,
 and 5547 for a server.
 .It Fl s Ar address
 Specify
-.A address
+.Ar address
 as the listening address of the process.
 The default address used when unspecified is ::1.
 .El
@@ -183,10 +182,10 @@ information (if any) and exits.
 .El
 .\"
 .Sh FILES
-.Bl -tag -width /usr/local/etc/dhcp6cctlkey -compact
-.It Pa /usr/local/etc/dhcp6cctlkey
+.Bl -tag -width /etc/wide-dhcpv6/dhcp6cctlkey -compact
+.It Pa /etc/wide-dhcpv6/dhcp6cctlkey
 is the default key file to communicate with a client.
-.It Pa /usr/local/etc/dhcp6sctlkey
+.It Pa /etc/wide-dhcpv6/dhcp6sctlkey
 is the default key file to communicate with a server.
 .El
 .\"
diff --git a/dhcp6relay.8 b/dhcp6relay.8
index 4f761b0..7ad8ada 100644
--- a/dhcp6relay.8
+++ b/dhcp6relay.8
@@ -107,7 +107,6 @@ to dump the process ID of
 is the default file that contains pid of the currently running
 .Nm .
 .El
-
 .Sh SEE ALSO
 .Xr dhcp6c 8 ,
 .Xr dhcp6s 8
diff --git a/dhcp6s.8 b/dhcp6s.8
index 888117a..29dcc7b 100644
--- a/dhcp6s.8
+++ b/dhcp6s.8
@@ -102,7 +102,7 @@ Use
 to store the shared secret to authenticate the communication with
 .Nm dhcp6ctl .
 The default file name used when unspecified is
-.Pa /usr/local/etc/dhcp6sctlkey .
+.Pa /etc/wide-dhcpv6/dhcp6sctlkey .
 The default name is intentionally same as that for
 .Nm dhcp6ctl
 so that the server and the control command can share the file when
@@ -122,12 +122,12 @@ to dump the process ID of
 .El
 .\"
 .Sh FILES
-.Bl -tag -width /usr/local/etc/dhcp6s.conf -compact
-.It Pa /usr/local/etc/dhcp6s.conf
+.Bl -tag -width /etc/wide-dhcpv6/dhcp6s.conf -compact
+.It Pa /etc/wide-dhcpv6/dhcp6s.conf
 is the default configuration file.
-.It Pa /var/db/dhcp6s_duid
+.It Pa /var/lib/dhcpv6/dhcp6s_duid
 is the default file to store the server's DUID.
-.It Pa /usr/local/etc/dhcp6sctlkey
+.It Pa /etc/wide-dhcpv6/dhcp6sctlkey
 is the default key file to communicate with the control command.
 See
 .Xr dhcp6ctl 8
diff --git a/dhcp6s.conf.5 b/dhcp6s.conf.5
index 1206764..2cb08ce 100644
--- a/dhcp6s.conf.5
+++ b/dhcp6s.conf.5
@@ -36,7 +36,7 @@
 .Nd DHCPv6 server configuration file
 .\"
 .Sh SYNOPSIS
-.Pa /usr/local/etc/dhcp6s.conf
+.Pa /etc/wide-dhcpv6/dhcp6s.conf
 .\"
 .Sh DESCRIPTION
 The
-- 
1.5.6.5

